For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to General Vehicle Lifting and Jacking in General Information.
2. Support the vehicle on a suitable stand.
3. Remove the pan. Refer to Oil Pan Replacement .
4. Remove the oil scoop retaining bolt.
5. Remove the oil scoop.

### Installation Procedure

1. Install the oil scoop.
2. Install the retaining bolt.

Tighten
Tighten the bolt to 8 N·m (71 lb in).

Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
3. Install the pan. Refer to Oil Pan Replacement .
4. Lower the vehicle.
5. Adjust the fluid level.