For 1990-2009 cars

### Removal Procedure

1. Remove the side upper garnish molding from the windshield. Refer to Garnish Molding Replacement - Upper .
2. Remove the screws from the floor carpet retainer.
3. Remove the floor carpet retainer.

### Installation Procedure

1. Install the floor carpet retainer.
2. Install the screws to the floor carpet retainer.
3. Install the side upper garnish molding to the windshield. Refer to Garnish Molding Replacement - Upper .