For 1990-2009 cars

# CLUNK NOISE: STEER. INT. SHAFT INT. SHAFT SLIP JOINT MOTION

#### MODELS AFFECTED: 1983-84 CENTURY AND SKYLARK

The labor time allowance to perform the "Clunk" Noise in Steering Intermediate Shaft repair as noted in Bulletin 84-3-9 dated Aug. '84 is as follows:

#### Labor Time Allowance

Labor Operation: T4084 Labor Time: .7 hr. Trouble Code: 92

Please update Service Bulletin 84-3-9 accordingly.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.