For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lock. Refer to Rear Compartment Lid Latch Replacement .
2. Slide out the retainer (1).
3. Remove the lock cylinder (2) and the gasket (1).

### Installation Procedure

1. Install the lock cylinder (2). Ensure that the following conditions are met:

• | The gasket (1) is in place

• | The lock cylinder engages with the cable remote connector.

2. Install the retainer (4) to the lock cylinder (2) on the rear compartment lid.
3. Install the rear compartment lock. Refer to Rear Compartment Lid Latch Replacement .