For 1990-2009 cars

#### Illuminated Entry Lamps Inoperative

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 | Using a fused jumper, connect RKE Module connector C1, terminal S, to ground. Do the interior lamps light? | -- | Go to Remote Keyless Entry System Check | Go to Step 3
3 | Inspect CKT 156 and CKT 1732. Refer to Interior Lights Schematics in Lighting Systems. Did you find and repair a condition? | -- | Go to Remote Keyless Entry System Check | --

#### Rear Compartment Lid Release Is Not Operable from Transmitters

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 | Using a fused jumper, connect RKE Module connector C1, terminal G, to battery voltage. Does the rear compartment lid release open? | -- | Go to Step 3 | Go to Step 4
3 | Inspect CKT 56. Did you find and repair a condition? | -- | Go to Step 5 | Go to Step 4
4 | Replace the rear compartment lid release solenoid. Is the replacement complete? | -- | Go to Step 5 | --
5 | Inspect for continuity at RKE Module connector C1, terminal K, with the transaxle in PARK or NEUTRAL (Automatic Transaxle) or with the park brake set (Manual Transaxle). Is continuity present? | -- | Go to Step 7 | Go to Step 6
6 | Inspect the relevant circuit. Refer to Keyless Entry Schematics . Did you find and repair a condition? | -- | Go to Step 7 | --
7 | Measure the voltage at RKE Module connector C1, terminal J with the ignition switch in RUN. Is the voltage present? | -- | Go to Remote Keyless Entry System Check | Go to Step 8
8 | Inspect CKT 39. Did you find and repair a condition? | -- | Go to Remote Keyless Entry System Check | --

#### All Transmitters are Inoperative or Partially Inoperative

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 | Using a fused jumper, connect RKE module connector C1, terminal A, to battery voltage. Does the driver's door unlock? | -- | Go to Step 5 | Go to Step 3
3 | Inspect CKT 694 and CKT 295. Did you find and repair a condition? | -- | Go to Step 5 | Go to Step 4
4 | Replace the left front door lock motor. Is the replacement complete? | -- | Go to Step 5 | --
5 | Measure the voltage at RKE module connector C1, terminal B, with either door lock switch held in the unlock position. Is the voltage present? | -- | Go to Step 7 | Go to Step 6
6 | Inspect CKT 194. Did you find and repair a condition? | -- | Go to Step 7 | --
7 | Measure the voltage at RKE module connector C1, terminal E. Is the voltage present? | -- | Go to Step 9 | Go to Step 8
8 | Repair the open in CKT 40. Is the repair complete? | -- | Go to Step 9 | --
9 | Using a fused jumper, connect RKE module connector C1, terminal G, to battery voltage. Does the rear compartment lid release open? | -- | Go to Step 10 | Go to Step 11
10 | Inspect CKT 56. Did you find and repair a condition? | -- | Go to Step 12 | Go to Step 11
11 | Replace the lid release solenoid rear compartment. Refer to Rear Compartment Lid Lock Cylinder Replacement in Body Rear End. Is the replacement complete? | -- | Go to Step 12 | --
12 | Using a fused jumper, connect RKE module connector C1, terminal S, to ground. Do the interior lamps light? | -- | Go to Step 14 | Go to Step 13
13 | Inspect CKT 156 and CKT 1732. Refer to Interior Lights Schematics in Lighting Systems. Did you find and repair a condition? | -- | Go to Step 14 | --
14 | Measure the voltage at RKE module connector C1, terminal R, with either door lock switch held in the lock position. Is the voltage present? | -- | Go to Step 16 | Go to Step 15
15 | Inspect CKT 195. Did you find and repair a condition? | -- | Go to Step 16 | --
16 | Inspect for continuity at RKE module connector C1, terminal N. Is continuity present? | -- | Go to Step 18 | Go to Step 17
17 | Inspect CKT 150. Did you find and repair a condition? | -- | Go to Step 18 | --
18 |

1. Inspect for continuity between RKE module connector C1, terminal L, and program connector C2, terminal A.
2. Connect RKE module connector C1, terminal L, to ground.

Is continuity present in the first case, and an open circuit present in the second case?

--

Go to Step 20

Go to Step 19

19 | Inspect CKT 1455. Did you find and repair a condition? | -- | Go to Step 20 | --
20 | Inspect for continuity at RKE module connector C1, terminal K, with the transaxle in PARK or NEUTRAL (Automatic Transaxle) or the park brake set (Manual Transaxle). Is continuity present? | -- | Go to Step 22 | Go to Step 21
21 | Inspect the relevant circuit. Refer to Keyless Entry Schematics . Did you find and repair a condition? | -- | Go to Step 22 | --
22 | Measure the voltage at RKE module connector C1, terminal J. Is the voltage present? | -- | Go to Remote Keyless Entry System Check | Go to Step 23
23 | Inspect CKT 39. Did you find and repair a condition? | -- | Go to Remote Keyless Entry System Check | --

#### Both Transmitters Operate System - Close Range Only

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 |

1. Inspect the battery in each transmitter.
2. Inspect the battery terminals in each transmitter.

Did you find and repair the condition?

--

Go to Remote Keyless Entry System Check

Go to Step 3

3 | Replace the remote control door lock receiver. Refer to Receiver Replacement . Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --

#### One Transmitter is Inoperative, Remaining Transmitters are OK

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 |

1. Inspect the battery in each transmitter.
2. Inspect the battery terminals in each transmitter.

Did you find and repair the condition?

--

Go to Remote Keyless Entry System Check

Go to Step 3

3 | Replace the remote control door lock receiver. Refer to Receiver Replacement . Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --

#### Driver's Door Cannot Be Locked from Door Lock Switch

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Remote Keyless Entry System Check? | -- | Go to Step 2 | Go to Remote Keyless Entry System Check
2 | Using a fused jumper, connect RKE module connector C1, terminal A, to battery voltage. Does the driver's door unlock? | -- | Go to Step 4 | Go to Step 3
3 | Inspect CKT 694 and CKT 295. Did you find and repair a condition? | -- | Go to Remote Keyless Entry System Check | Go to Step 4
4 | Replace the left front door lock motor. Is the repair complete? | -- | Go to Remote Keyless Entry System Check | --