For 1990-2009 cars

### Removal Procedure

1. Remove the shoulder belt guide bolt from the driver side or the passenger side.
2. Grasp the upper trim finish panel on the center pillar and pull.
3. Remove the upper trim finish panel from the center pillar.
4. Remove the side upper garnish molding from the windshield. Refer to Garnish Molding Replacement - Upper .

### Installation Procedure

1. Install the side upper garnish molding on the windshield. Refer to Garnish Molding Replacement - Upper .
2. Install the upper trim finish panel to the center pillar.
3. Install the shoulder belt guide bolt to the driver side or the passenger side.