For 1990-2009 cars

### Removal Procedure

1. Remove the screws that retain the flexible splash shield from forward of the left front wheel.
2. Remove the screws that retain the fog lamp relay.
3. Remove the fog lamp relay connector.

### Installation Procedure

1. Install the fog lamp relay connector to the fog lamp relay.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws that retain the fog lamp relay to the fender.

Tighten
Tighten the screw to 10 N·m (89 lb in).

3. Install the screws that retain the flexible splash shield.