For 1990-2009 cars

# 75MM OIL FILTER (SMALL) INSTALLATION INFORMATION

#### SUBJECT: 75MM OIL FILTER INSTALLATION TO PREVENT LEAKAGE OF SMALL 75MM OIL FILTERS SUCH AS PF40, PF45, PF47, PF51, ETC., IT IS VERY IMPORTANT THAT THE INSTALLATION INSTRUCTIONS ON THE LABEL ARE CLOSELY FOLLOWED. IF THE FILTER CANNOT BE TIGHTENED BY HAND THE CORRECT AMOUNT OF TURNS SPECIFIED ON THE LABEL AFTER GASKET CONTACT, IT IS RECOMMENDED THAT A CAP WRENCH SUCH AS OF17W BE USED.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.