For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 28733-A Front Hub Spindle Remover.

1. Remove the drive axle nut. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
2. Remove the brake caliper bolts and support the caliper. Refer to Brake Caliper Replacement in Disc Brakes.
3. Remove the rotor. Refer to Brake Rotor Replacement in Disc Brakes.
4. Remove the rotor. Refer to Brake Rotor Replacement . Disconnect the ABS sensor harness connector from the retaining bracket and wiring harness.
5. Remove the hub and bearing assembly (1) from the steering knuckle (2).

### Installation Procedure

1. Install the hub and bearing assembly (1) to the steering knuckle (2).
2. Connect the ABS sensor harness connector from the retaining bracket and wiring harness.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the hub and bearing assembly bolts (5).

Tighten
Tighten the hub and bearing assembly bolts to 95 N·m (70 lb ft).

4. Install the rotor. Refer to Brake Rotor Replacement in Disc Brakes.
5. Install the brake caliper and the bolts. Refer to Brake Caliper Replacement in Disc Brakes.
6. Install the drive axle nut. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
7. Check the front wheel alignment. Refer to Wheel Alignment Specifications in Wheel Alignment.