For 1990-2009 cars

### Removal Procedure

1. Remove the RH engine splash shield (wheel house panel).
2. Disconnect the hoses from the EVAP canister.
3. Remove the EVAP canister retainer attaching bolt (1).
4. Remove the EVAP canister (2) and retainer (3).

Notice: The EVAP canister may have released carbon particles which caused this part to fail and may cause damage to other components. Check the EVAP canister for loose carbon before returning the vehicle to service.

5. Remove the EVAP canister retainer (3) from the canister (2).

### Installation Procedure

1. Snap the EVAP canister retainer (3) onto the EVAP canister (2).

Important: When installing the EVAP retainer to the EVAP canister, the attaching bolt must be towards the front of the vehicle and the hose ports must be towards the rear of the vehicle.

2. Install the rearward end of the EVAP canister retainer (3) into the slot in the PCM bracket (rotate the EVAP canister to insert the top of the EVAP canister under the tab on the PCM bracket).
3. Install the EVAP canister retainer attaching bolt (1).

Tighten
Tighten the EVAP canister retainer attaching bolt to 10 N·m (88 lb in).

4. Connect the hoses to the EVAP canister.
5. Install the RH engine splash shield (wheel house panel).