For 1990-2009 cars

# CAMSHAFT SPROCKET TO CAM TORQUE SPECIFICATIONS

1988 2.3 QUAD 4 (VIN CODE D) CAMSHAFT SPROCKET TO CAM TORQUE SPECIFICATION

#### VEHICLES AFFECTED: 1988 N SERIES WITH 2.3 QUAD 4 ----------------- (VIN CODE D) ENGINE

The cam sprocket to cam bolt torque specification was omitted from the 1988 New Product Service Manual (Page 6A7-19, Step 14 and Page 6A7-40).

The correct torque is 50 Nm or 37 ft. lbs.

Please note this specification in your 1988 Cutlass Calais New Product Service Manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.