For 1990-2009 cars

## Front Bumper Fascia Replacement Pontiac

### Removal Procedure

1. Partially remove the right and the left front wheelhousings. Refer to Wheelhouse Panel Replacement in Body Front End.
2. Remove the headlamp assemblies in order to access the bolts.
3. Remove the retainers (1) which connect the fascia (3) to the impact bar.
4. Remove the bolts (1) which connect the fascia (2) to the fender.
5. Remove the front bumper fascia (3) from the impact bar.

### Installation Procedure

1. Install the fascia (3) to the impact bar.
2. Install the bolts (1) attaching the fascia (2) to the fender.
3. Attach the fascia (3) by installing retainers (1) through the holes (2) in the impact bar.
4. Install the headlamp assemblies.
5. Install the wheelhousings.

## Front Bumper Fascia Replacement Buick and Oldsmobile

### Removal Procedure

1. Partially remove the right and the left front wheelhousings. Refer to Wheelhouse Panel Replacement in Body Front End.
2. Remove the headlamp assemblies in order to access the bolts.
3. Remove the retainers (1) which connect the fascia (3) to the impact bar.
4. Remove the bolts (1) which connect the fascia (2) to the fender.
5. Remove the front bumper fascia (3) from the impact bar.

### Installation Procedure

1. Install the fascia (3) to the impact bar.
2. Install the bolts (1) attaching the fascia (2) to the fender.
3. Attach the fascia (3) by installing retainers (1) through the holes (2) in the impact bar.
4. Install the headlamp assemblies.
5. Install the wheelhousings.