For 1990-2009 cars

# OIL LEAK AT OIL PAN DRAIN PLUG V-8, V6, OHV L4 CARS & TRUCKS

NEW OIL DRAIN PLUG GASKET TO REPLACE COPPER GASKET

#### MODELS AFFECTED: ALL 1986 AND PAST MODEL YEAR APPLICATIONS OF 2.0L --------------- L-4 (VIN P) AND 2.8L V-6 (VIN W AND X) ENGINES

An improved oil drain plug gasket, Part No. 14090908, is available to replace the copper gasket, Part No. 14079550. The new gasket is a steel washer with captured O-Ring (Viton).

The new O-Ring/Steel gasket is capable of sealing irregular surfaces with light torques while retaining the clamping load over time. Reuse of the O- Ring/Steel gasket does not lessen sealing or torque retention characteristics.

Recommended torque for the O-Ring/Steel gasket is 12-20 lb. ft. (16-27 N.m)

Excessively higher torques may cause deformation, splitting, or loss of sealing capability.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.