For 1990-2009 cars

# FRT SIDE DOOR ARMREST MOLDING RETENTION (APPLY ADHESIVE)

#### SUBJECT: FRONT SIDE DOOR ARMREST MOLDING RETENTION (APPLY ADHESIVE)

#### MODELS AFFECTED: 1992-93 SKYLARK MODELS

#### CONDITION:

Some owners of 1992-93 Skylarks may comment that the front side door armrest molding does not stay fully seated in the door trim panel.

#### CAUSE:

Front side door armrest molding barbs have been damaged and no longer retain the molding.

#### CORRECTION:

1. Pull the molding away from the upper trim panel in the affected area.

2. Apply a drop of adhesive, P/N 12345632, or equivalent on the top side of the molding barbs and reinsert the barbs into the slots.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation Number: T1891 Labor Time: 0.2 Hour (Both sides)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.