For 1990-2009 cars

### Removal Procedure

1. Disable the supplemental inflatable restraint (SIR) system. Refer to Disabling the SIR System in SIR.
2. Open the access door and disconnect the yellow 2-way air bag wire.
3. Using locking pliers and a protective covering, remove the tilt lever. Refer to Tilt Lever Replacement - On Vehicle in Steering Wheel and Column - Tilt.
4. Remove the column shift boot (1).
5. Remove the 5 screws and the upper and lower steering column covers.
6. Remove the 3 Torx® screws (3) and the shift lever assembly (2).

### Installation Procedure

1. Install the 3 Torx® screws (3) and the shift lever assembly (2).
2. Install the 5 screws and the upper and lower steering column covers.
3. Install the column shift boot (1) with the angled end (4) at the top.
4. Using locking pliers and a protective covering, install the tilt lever.
5. Connect the yellow 2-way air bag wire and close the access door.
6. Enable the SIR system. Refer to Enabling the SIR System in SIR.