For 1990-2009 cars

# SERVICE MANUAL UPDATE - SPEC. REVISION (NEW ARTWORK)

#### SUBJECT: SERVICE MANUAL UPDATE - TORQUE SPECIFICATION REVISION (NEW ARTWORK) FOR LOWER ENGINE MOUNT STRUT

#### MODELS AFFECTED: 1992-93 SKYLARKS WITH 2.3L (VIN 3-RPO L40)

This is a service manual update to Sections 6A6 and 6A7.

The torque specification for the lower engine mount strut has been revised. Refer to the artwork on the following pages:

1992 Skylark, Page 6A6-10, Figure 11 - Update with Figure 1 Page 6A7-11, Figure 12 - Update with Figure 1

1993 Skylark, Page 6A7-11, Figure 12 - Update with Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.