For 1990-2009 cars

# IMPRESSION IN DOOR FORWARD OF THE DOOR HANDLE (INST. PANEL)

#### SUBJECT: IMPRESSION IN DOOR FORWARD OF THE DOOR HANDLE (INSTALL REINFORCEMENT PANEL)

#### MODELS: 1992-93 BUICK SKYLARK 1992-93 PONTIAC GRAND AM (VEHICLES AFFECTED ARE COUPES ONLY)

#### CONDITION:

SOME OWNERS MAY COMMENT ON AN IMPRESSION IN THE DOOR FORWARD OF THE DOOR HANDLE.

#### CAUSE:

PRESSURE APPLIED FORWARD OF THE DOOR HANDLE DEFORMS DOOR OUTER SHEET METAL.

#### CORRECTION:

1. REMOVE DOOR TRIM PANEL, REFER TO SECTION 10-6 IN THE SERVICE MANUAL.

2. REMOVE WATER DEFLECTOR ENOUGH TO REPAIR IMPRESSION AND INSTALL DOOR REINFORCEMENT PANEL.

3. REMOVE ENOUGH SOUND DEADENING PATCH TO REPAIR IMPRESSION AND INSTALL DOOR REINFORCEMENT PANEL.

4. REPAIR IMPRESSION IN DOOR.

5. PEEL OFF TAPE BACKING FROM DOOR REINFORCEMENT PANEL.

6. INSTALL DOOR REINFORCEMENT PANEL, P/N 22597410. SEE FIGURE 1.

7. INSTALL WATER DEFLECTOR.

8. INSTALL DOOR TRIM PANEL, REFER TO SECTION 10-6 IN THE SERVICE MANUAL.

PARTS ARE EXPECTED TO BE AVAILABLE ON JUNE 20, 1994.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: B4298 (RIGHT DOOR) B4299 (LEFT DOOR) LABOR TIME: 0.7 HR. (EACH DOOR)

FIGURES: 1

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.