For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement .
2. Place the rear seat cushion on a clean, dry and non-abrasive surface.
3. Remove the hog rings.
4. Remove the rear seat cushion cover.

### Installation Procedure

1. Install the rear seat cushion cover.
2. Fold the cover over at the bolster line in order to expose the locating holes. Match the alignment holes in the cover to the alignment marks on the pad in order to align the cover.
3. Engage the hook and loop strips by running your hand along the total length of the bolster areas.
4. Install the hog rings.
5. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement .