For 1990-2009 cars

## Front Bumper Lower Fascia Grille Replacement Pontiac

### Removal Procedure

1. Remove the grille screws (4).
2. Disengage the grille tabs (3) from the slots (1).
3. Remove the grille (2).

### Installation Procedure

1. Install the grille by inserting the tabs (3) into the slots (1).
2. Engage the grille tabs (3) to the slots (1).
3. Install the grille screws (4).

## Front Bumper Lower Fascia Grille Replacement Buick

### Removal Procedure

1. Remove the grille screws (4).
2. Disengage the grille tabs (2) from the slots (5).
3. Remove the grille (3).

### Installation Procedure

1. Install the grille (3) by inserting the tabs (2) into the slots (5).
2. Engage the grille tabs (2) to the slots (5).
3. Install the grille screws (4).