For 1990-2009 cars

# INTERMITTENT ELECT CONDITIONS (REPAIR/REROUTE ENG. HARNESS)

#### SUBJECT: INTERMITTENT ELECTRICAL CONDITIONS (REPAIR/REROUTE ENGINE HARNESS)

#### MODELS AFFECTED: 1992-93 SKYLARK

#### CONDITION:

--------- Some owners of 1992-93 Skylarks may comment that the car exhibits one or more of the following conditions:

- will not start/stalls

- coolant fan inoperable/engine overheats

- coolant fan always on/ will not turn off

- ABS indicator light on

- engine vent heater inoperable

- air conditioning inoperable

- rear window defogger inoperable

- power seats inoperable

- horn inoperable

- instrument panel malfunctions/does not light

- cigar lighter inoperable

- remote keyless entry inoperable

- transaxle converter clutch inoperable

- power mirrors inoperable

#### CAUSE:

----- Relay wires may be routed too closely to the Transmission Fluid Indicator (V6 application only) or the Brake Booster (all engines). Wire chafing may occur, possibly causing some of the conditions listed above.

#### CORRECTION:

---------- Repair chafed wiring and cover all relay leads with additional conduit and tape. Reroute harness area away from Brake Booster and/or Transmission Fluid Indicator to prevent further chaffing.

#### WARRANTY INFORMATION:

Labor Operation Number: T1924

Labor Time: 0.6 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.