For 1990-2009 cars

Table 1: | ABS Motor Pack Assembly
Table 2: | Brake Switch
Table 3: | Electronic Brake Control Relay
Table 4: | Electronic Brake Control Module

#### ABS Motor Pack Assembly

Connector Part Information |

• | 12160746

• | 6-Way F Metri-Pack Series 280 FLX LK (LT GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1280 | ABS Motor Feed-Left Front
B | PNK | 1281 | ABS Motor Return-Left Front
C | DK GRN | 1284 | ABS Motor Feed-Rear
D | ORN | 1285 | ABS Motor Return-Rear
E | PPL | 1282 | ABS Motor Feed-Right Front
F | BLK | 1283 | ABS Motor Return-Right Front

#### Brake Switch

Connector Part Information |

• | 12033701

• | 2-Way F Metri-Pack Series 480 (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 140 | Fuse Output-Battery
B | LT BLU | 20 | Stop Lamp Feed

#### Electronic Brake Control Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack Series 280 FLX LK (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | RED | 342 | Switched Battery Voltage Input
85 | PNK | 1632 | Coil Side Output
86 | PNK | 439 | Coil Side Input
87 | RED | 1633 | Switched Battery Voltage Output

#### Electronic Brake Control Module

Connector Part Information |

• | 12160423

• | 32-Way F Metri-Pack Series 280 Micro-Pack Series 100 W (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GRA | 1056 | Steering Wheel Position Sensor Feed - 5 Volt Reference
2 | PNK | 1632 | ABS Enable Relay Output - Coil
3 | GRN DK | 1288 | ABS Isolation Solenoid Feed - Left Front
4 | PNK | 439 | Fuse Output - Ignition 1 - Type III Fuse
5 | ORN/BLK | 556 | Steering Wheel Position Sensor Return
8 | BLU LT | 830 | Wheel Speed Sensor Signal - Left Front
9 | GRN DK | 872 | Wheel Speed Sensor Signal - Right Front
10 | BLK | 884 | Wheel Speed Sensor Signal - Left Rear
11 | BRN | 882 | Wheel Speed Sensor Signal - Right Rear
12 | TAN | 800 | Serial Data Signal - UART - 8192 Baud - Primary
13 | ORN | 340 | Fuse Output - Battery - Type III Fuse
16 | WHT | 17 | Stop Lamp Switch Output
17 | BLU LT | 1059 | Steering Wheel Position Sensor Signal
18 | BRN | 1295 | Electronic Variable Orifice Solenoid Output
19 | BLU LT | 1289 | ABS Isolation Solenoid Feed - Right Front
20 | PNK | 849 | Brake Fluid Level Sensor Signal
21 | YEL | 873 | Wheel Speed Sensor Return - Left Front
22 | TAN | 833 | Wheel Speed Sensor Return - Right Front
23 | RED | 885 | Wheel Speed Sensor Return - Left Rear
24 | WHT | 883 | Wheel Speed Sensor Return - Right Rear
A | PPL | 1282 | ABS Motor Feed - Right Front
B | BLK | 1283 | ABS Motor Return - Right Front
C | RED | 1633 | ABS Enable Relay Output - N.O Contact
D | BLK | 250 | Ground
E | ORN | 1285 | ABS Motor Return - Rear
F | GRN DK | 1284 | ABS Motor Feed - Rear
G | BLK | 1280 | ABS Motor Feed - Left Front
H | PNK | 1281 | ABS Motor Return - Left Front