For 1990-2009 cars

### Removal Procedure

1. Relieve fuel system pressure. Refer to Fuel Pressure Relief .
2. Drain fuel tank. Refer to Fuel Tank Draining .
3. Remove the fuel tank. Refer to Fuel Tank Replacement .
4. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
5. Note strainer position (1) for future reference.
6. Support the reservoir with one hand and grasp the strainer with the other hand.
7. Using a screwdriver to pry the strainer ferrule off the reservoir.
8. Discard the strainer.

### Installation Procedure

1. Install the new strainer (1) to reservoir.
2. Support the reservoir with one hand and grasp the strainer with the other hand twisting the strainer into position.
3. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
4. Reinstall the fuel tank. Refer to Fuel Tank Replacement .
5. Refill tank and reinstall the fuel fill cap.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

6. Reconnect the negative battery cable.
7. Check for fuel leaks.

7.1. | Turn the ignition switch ON for 2 seconds.

7.2. | Turn the ignition switch OFF for 10 seconds.

7.3. | Turn the ignition switch ON.

7.4. | Check for fuel leaks.