For 1990-2009 cars

# ENGINE OIL RECOMMENDATIONS PREFERRED VISCOSITIES

#### MODELS AFFECTED: ALL PASSENGER CARS

The purpose of this bulletin is to:

- Advise you of the reasons for changes in engine oil viscosity recommendations, and

- Explain the new API service synbol which should assist vehicle owners in finding engine oils recommended for cut engines.

#### Gasoline Engine Oil Viscosity Recommendations

Since 1980, the preferred viscosities for GM gasoline engines are SAE 10W-30 for the larger engines and SAE 5W-30 for the smaller engines (engines sizes defined later).

SAE 10W-40 is not included in the viscosity chart for 1984 GM gasoline engines, for several reasons, including:

- Fuel economy with SAE 10W-30 oils is about 1 percent better than that with SAE 10W-40 oils.

- SAE 10W-30 oils generally produce less piston and ring deposits than SAE 10W-40 oils. Such deposits can lead to stuck rings and increased oil consumption.

The use of SAE 10W-40 erigine oil in a vehicle equipped with a gasoline engine will not automatically void the General Motors Corporations New Car Limited Warranty. However, since SAE 10W-40 engine oil is not recommended for use in 1984 (24 vehicles equipped with gasoline engines, if the use of such oil causes damage, the cost of the engine repair will not be covered by the Warranty. The Warranty does not cover any damage due to the use of non-recommended oils, whether SAE 10W-40 or some other viscosity. In addition, the Warranty does not cover damages caused by the use of oils that do not meet the recommended API quality of SAE viscosity grade.

#### Diesel Engine Oil Viscosity Recommendations

Preferred viscosities for diesel engines in GM passenger cars are SAE 30 for the larger engines and SAE 10W-30 for the smaller engines.

SAE 10W-40 oils have never been recommended for diesel engines in GM passenger cars. Nevertheless, some owners have used SAE10W-40 oils and, in some cases, experienced engine damage caused by excessive piston and ring deposits. In an effort to clarify the GM recommendations for passenger cars, the 1984 owner's manuals state specifically for diesel engines "DO NOT USE SAE 1-W-40 CRADE OIL, OR ANY OTHER GRADE NOT RECOMMENDED."

If damage to a GM diesel engine is caused by the use of SAE 10W-40 engine oil, the cost of the engine repair will not be covered by the Warranty.

API Engine Oil Service Symbol

A new API service symbol is being used in GM owner's manuals and on oil cans. Urge your customers to look for it in their manuals and on the containers of the oil they select for use in their cars. These are examples of the symbol:

Small Gasoline Larger Gasoline Larger Diesel Engines (3.0L and larger V-6 Engines (4 cyl & 2.8L, V-6) and V-8) and (4.3L, 5.7 & 6.2L) Small Diesel (1.8L & 2.2L) Engines

The symbol has an upper segment, center area, and lower segment. An explanation of the information in each of these locations is as follows:

UPPER SEGMENT: QUALITY LEVEL ------------------------------ API (American Petroleum Institute) Service Categories

Gasoline Engines Diesel Engines ---------------- --------------- SF/CC SF/M (preferred) SF/M SF/CC SF

CENTER AREA: OIL THICKNESS (Grade) ---------------------------------- SAE (Society of Automotive Engineers) Viscosity Classification

Gasoline Engines Diesel Engines ----------------- --------------- SAE 5W-30 (preferred for SAE 30 (preferred abave engines of 2.8 liters or less) freezing*).

SAE 10W-30 (preferred for SAE 10W-30 and SAE 1514-40 all other engines). (acceptable for all engines; use only for cold-weather SAE 15W-40, SAE 20W-20 and operations; helps starting). SAE 30 (acceptable for all engines). * Except for 1.8 and 2.2 liter diesels, where SAE 10W-30 is preferred at all temperatures.

LOWER SEGMENT: FUEL ECONOMY RATING -------------- "ENERGY CONSERVING"

Oils with these words provide more miles per gallon of fuel.

The Goodwrench line of engine oils recently introduced by GM meets these standards and provides proper lubrication protection for passenger cars.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.