For 1990-2009 cars

## Exhaust Manifold Installation Left Side

1. Install the exhaust manifold gasket.
2. Install the exhaust manifold.
3. Install the exhaust manifold nuts.

Tighten
Tighten the exhaust manifold nuts to 16 N·m (12 lb ft).

Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
4. Install the exhaust manifold heat shield.
5. Install the exhaust manifold heat shield nuts.

Tighten
Tighten the exhaust manifold heat shield nuts to 10 N·m (89 lb in).

## Exhaust Manifold Installation Right Side

1. Install the exhaust manifold gasket.
2. Install the exhaust manifold. Loosely, install the heat shield at this time.
3. Install the exhaust manifold nuts.

Tighten
Tighten the exhaust manifold nuts to 16 N·m (12 lb ft).

Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
4. Install the exhaust manifold heat shield.
5. Install the exhaust manifold heat shield nuts.

Tighten
Tighten the exhaust manifold heat shield nuts to 10 N·m (89 lb in).

6. Install the converter heat shield to the body.
7. Install the exhaust pipe to the converter flange.
8. Install the heated oxygen sensor.
9. Install the crossover pipe to the exhaust manifolds.
10. Install the crossover heat shield.
11. Install the EGR pipe to the exhaust manifold.