For 1990-2009 cars

# SQUAWK/CLUNK NOISE FROM FRT. SUSP.-REPLACE STABILIZER BUSH.

#### SUBJECT: SQUAWK/CLUNK NOISE FROM FRONT SUSPENSION (REPLACE STABILIZER BUSHINGS WITH NEWER DESIGNED BUSHINGS)

#### VEHICLES AFFECTED: 1985-91 J/N/L/ CARS

#### CONDITION:

----------- Some 1985-91 J/N/L cars might exhibit a condition of a "Squawk" OR "Clunk" noise from the front suspension or engine compartment area when driving over small bumps or entering parking lots (i.e. washboard road surfaces, railroad tracks).

#### CAUSE:

------- The condition may be caused by the rubber bushing material bleeding through the teflon/polyester sock and coming into contact with the stabilizer bar.

#### CORRECTION:

------------ If this condition is encountered, replace both stabilizer bar bushings with newer designed bushings. The part numbers for the new bushings are listed below:

STABILIZER BAR DIAMETER BUSHING PART NUMBER(S) ----------------------- ----------------------- 22mm 22566673 24mm 22566674 26mm 22566675 28mm 22553016 30mm 10088389

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.