For 1990-2009 cars

The Powertrain Control Module (PCM) controls the following items:

• | Fuel metering system.

• | Transaxle shifting.

• | Ignition timing.

• | On-board diagnostics for Powertrain functions.

It constantly looks at the information from various sensors, and controls the systems that affect vehicle performance. The PCM also performs the diagnostic function of the system. It can recognize operational problems, alert the driver through the MIL (Service Engine Soon), and store diagnostic trouble codes which identify the problem areas to aid the technician in making repairs.

#### PCM Function

The PCM supplies either 5 or 12 volts to power various sensors or switches. This is done through resistances in the PCM which are so high in value that a test light will not light when connected to the circuit. In some cases, even an ordinary shop voltmeter will not give an accurate reading because its resistance is too low. Therefore, a digital voltmeter with at least 10 megohms input impedance is required to ensure accurate voltage readings. Tool J 39200 meets this requirement. The PCM controls output circuits such as the injectors, IAC, cooling fan relays, etc. by controlling the ground or power feed circuit through transistors or a device called a Driver.

#### EEPROM

The Electrically Erasable Programmable Read Only Memory (EEPROM) is a permanent memory that is physically soldered within the PCM. The EEPROM contains program and calibration information that the PCM needs to control powertrain operation. Unlike the PROM used in certain past applications, the EEPROM is not replaceable. If the PCM is replaced, the new PCM will need to be programmed. Techline equipment (Tech-2) containing the correct program and calibration for the vehicle is required to program the PCM.