For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Check for hard or severe driving. Has the vehicle been driven severely? | -- | System OK | Go to Step 2
2 | Check for rotation of the tires. Have the tires been rotated? | -- | Go to Step 3 | Go to Tire Rotation
3 | Check for proper tire inflation pressure. Have the tires been inflated to the proper pressure level? | -- | Go to Step 4 | Go to Tire Repair
4 | Check for sagging or broken springs. Are the springs sagging or broken? | -- | Go to Spring Replacement in Front Suspension | Go to Step 5 .
5 | Check tires for proper balancing. Are the tires properly balanced? | -- | Go to Step 6 | Go to Tire Repair
6 | Check the condition of the strut dampener or shock absorber. Is the strut dampener or shock absorber worn? | -- | Go to Strut Assembly Replacement | Go to Step 7
7 | Check the vehicle for overloading. Is the vehicle overloaded? | -- | Remove the excess weight. | Go to Step 8
8 | Check for proper wheel alignment. Are the wheels properly aligned? | -- | System OK | Go to Wheel Alignment Specifications