For 1990-2009 cars

### Removal Procedure

1. Remove the 3 fasteners (4) from the upper quarter trim panel (3).
2. Slide the upper quarter trim panel back while you rotate the trim panel towards the front of the vehicle.
3. Remove the upper quarter trim panel (3).

### Installation Procedure

1. Install the upper quarter trim panel (3). Ensure that the front edge is inserted into the 2 slots (1) of the lower quarter trim panel.
2. Apply sufficient pressure to the panel in order to full seat the 3 fasteners (4).