For 1990-2009 cars

### Disassembly Procedure

1. Remove the wheel cylinder from the vehicle. Refer to Wheel Cylinder Replacement .
2. Remove the wheel cylinder boots (4).
3. Remove the wheel cylinder pistons (3) and seals (2).
4. Remove the wheel cylinder spring assembly (5).
5. Remove the wheel cylinder bleeder valve (6).
6. Inspect the cylinder bore (1) and pistons (3) for the following conditions:

• | Scoring

• | Nicks

• | Corrosion

• | Wear

7. Use a crocus cloth in order to polish out light corrosion. Replace the wheel cylinder assembly if the bore does not clean up using the crocus cloth.
8. Clean all the parts in clean, denatured alcohol.
9. Dry the parts with unlubricated, compressed air.

Caution: When servicing brake parts, do not create dust by grinding or sanding brake linings, by cleaning brake parts with a dry brush or with compressed air. Many earlier models or aftermarket brake parts may contain asbestos fibers which can become airborne if dust is created during servicing. Breathing dust containing asbestos fibers may cause serious bodily harm. A water dampened cloth or water based solution should be used to remove any dust on brake parts. Equipment is commercially available to perform this washing function. These wet methods will prevent fibers from becoming airborne.

Notice: Brake fluid will damage painted surfaces. Shop cloths and clean containers should be used to prevent spillage of brake fluid.

10. Lubricate the new seals (2) with clean brake fluid.

### Assembly Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the bleeder valve (6).

Tighten
Tighten the bleeder valve to 7 N·m (62 lb in).

2. Install the spring assembly (5).
3. Install the following components:

• | Seals (2)

• | Pistons (3)

• | Boots (4)

4. Install the wheel cylinder to the vehicle. Refer to Wheel Cylinder Replacement .