For 1990-2009 cars

# SQUEAK NOISE IN STEERING WHEEL LUBRICATE TILT WHEEL ASSEMBLY

#### MODELS AFFECTED: ALL WITH TILT STEERING COLUMNS

Some vehicles equipped with tilt or tilt and telescope steering columns may experience a squeaking noise when turning the steering wheel in a tilted position. This can be caused by insufficient grease in the tilting mechanism.

Step 1 - To Check For This Condition:

1. Start engine. 2. Position steering wheel in the full up position, Figure 1. 3. Touching only the rim (so the center pad does not cause a squeak), turn the steering wheel back and forth to the extreme left and right position. 4. Repeat this procedure at straight on position, and full down position.

Step 2 - To Repair This Condition:

1. Tilt steering wheel to full up position. 2. Spray lube, GM-1052349, lubriplate lubricant grease (or equivalent) into the opening, as shown in Figure 2, along side the tilt lever, aiming at the universal joint. Turn steering wheel one full turn while applying grease. 3. Hold tilt release lever in moveable position and move steering wheel from full up to full down position 4 to 8 times. 4. If squeak persists, repeat Step 2.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.