For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 29809 Tie Rod Bushing Remover and Installer

1. Remove the inner tie rod. Refer to Steering Linkage Inner Tie Rod Replacement .
2. Use J 29809 in order to remove the inner pivot bushing (1) from the inner tie rod (2).

### Installation Procedure

1. Coat the inner pivot bushing (1) with grease for easier installation.
2. Use J 29809 in order to install the inner pivot bushing (1) into the inner tie rod (2).
3. Install the center housing cover washer (6) until fitted into the rack and pinion boot (1).
4. Install the inner tie rod bolts (4) in the following manner:

4.1. | Through the holes in the bolt support plate (5)

4.2. | Through the inner pivot bushing that is part of the inner tie rod (2)

4.3. | Through the center housing cover washer (6) captured in recesses in the rack and pinion boot (1)

4.4. | Insert into the rack guide assembly, inside the rack and pinion boot (1)

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4.5. | Insert into the threaded hole in the rod and rack assembly

Tighten
Tighten the inner tie rod bolts to 90 N·m (65 lb ft).

5. Install the new lock plate (3) with the notches in the proper position over the flats of the inner tie rod bolts (4).