For 1990-2009 cars

# SERVICE MANUAL UPDATE-SEC. 0B COOLING SYSTEM CAPACITIES

#### MODELS AFFECTED: 1989-90 SKYLARK WITH 2.3L ENGINE (VIN CODE D), 2.5L ENGINE (VIN CODE U), AND 3.3L ENGINE (VIN CODE N)

THIS BULLETIN IS BEING ISSUED TO ADD 2.3L VIN CODE D AND REPLACES BULLETIN 90-0-4, DATED JUNE, 1990, WITH REFERENCE NUMBER 90-156-0.

The following is corrected engine cooling system coolant capacities.

2.3L (VIN D) - 9.8 Liters (10.4 Quarts) 2.5L (VIN U) - 10.1 Liters (10.7 Quarts) 3.3L (VIN N) - 12.0 Liters (12.7 Quarts)

Please mark a reference to this bulletin in your copy of the following service manual in Section OB, page OB-8, Maintenance and Lubrication, at the "Approximately Fluid Capacities" Chart:

1989 - 1990 Skylark

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.