For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Move the headlamp dimmer switch to LOW.
2. Turn the headlamp switch to HEAD.

The low beam headlamps are on.

Headlamps Inoperative - Low Beams

2 | Turn the headlamp dimmer switch to the HIGH position. |

• | The high beam headlamps are on.

• | The high beam indicator is lit.

• | The low beam headlamps are off.

Headlamps Inoperative - High Beams

3 |

1. Move the headlamp dimmer switch to LOW.
2. Hold the flash-to-pass switch on.

• | The high beam headlamps are on.

| The high beam indicator is lit.

• | The low beam headlamps are on.

• | Headlamps Inoperative - High Beams

• | Headlamps Inoperative - Low Beams

4 | Release the flash-to-pass switch. | The low beam headlamps are on. | Headlamps Inoperative - Low Beams
5 | Turn the headlamp switch to the OFF position. |

• | The high beam headlamps are off.

• | The high beam indicator is off.

Headlamps Inoperative - High Beams

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.