For 1990-2009 cars

# SMU - SECTION 6E3 - DRIVEABILITY & EMISSIONS

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION-6E3-DRIVEABILITY AND EMISSIONS- REVISED FIGURE A-7-PCM CONNECTOR TERMINAL END VIEW

#### MODELS: 1994-95 BUICK SKYLARK 1994-95 OLDSMOBILE ACHIEVA 1994-95 PONTIAC GRAND AM WITH 2.3L ENGINE (VINS A, D, 3 - RPOS LGO, LD2, L4O) AND 4T60-E TRANSAXLE

THIS BULLETIN IS BEING ISSUED TO CORRECT AN ERROR IN SECTION 6E3-A-8, FIGURE A-7-PCM CONNECTOR TERMINAL END VIEW.

THE CORRECTION IS AS FOLLOWS:

IN THE BLUE 32 PIN C-D CONNECTOR 3 (C-3) TABLE, SHIFT "B" (ROW BC14) AND SHIFT "A" (ROW BC15) ARE LABELED INCORRECTLY.

SHIFT "B" SHOULD BE IN ROW **BC15** AND SHIFT "A" SHOULD BE IN ROW **BC14**. THE VOLTAGES AND WIRE COLORS ARE CORRECT AS THEY ARE. PLEASE CORRECT YOUR SERVICE MANUAL ACCORDINGLY.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.