For 1990-2009 cars

### Removal Procedure

1. Remove the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.
2. Remove the speaker screws (3).
3. Disconnect the electrical connector (4).
4. Remove the speaker (2) from the rear shelf panel (1).

### Installation Procedure

1. Install the speaker (2) to the rear shelf panel (1).
2. Connect the electrical connector (4).
3. Install the speaker screws (3).
4. Install the rear window trim panel. Refer to Rear Window Trim Panel Replacement in Body Rear End.