For 1990-2009 cars

# DRIVE AXLE NUT SIZE USE OF DEEP WELL SOCKET

#### MODELS AFFECTED: 1984 CENTURY, SKYLARK, SKYHAWK, RIVIERA 1985 ELECTRA

When removing the drive axle nut on 1984-85 front-wheel-drive models it is advisable to use a 6-point deep well socket as listed below.

#### MODEL SOCKET SIZE ----- ------------ 1984 Century with JA1/JA8 30.0mm Brakes - See Service Parts Identificatim Label

1984 Century with JA2/JA3 36.0mm Brakes - See Service Parts Identification Label

1984 Skylark 30.0mm

1984 Skyhawk 30.0mm

1984 Riviera 36.0mm

1985 Electra 36.0mm

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.