For 1990-2009 cars

## Front Door Switch Replacement Left, Pontiac Coupe

### Removal Procedure

1. Remove the screws (5).
2. Remove the power lock and window switch bezel (2) from the door trim.
3. Disconnect the wire harness connector (1) from the power door lock switch (3).
4. Disconnect the wire harness connector (1) from the power door window switch (4).
5. Remove the power door lock switch (3) from the window switch bezel (2).
6. Remove the door window switch (4) from the power lock and window switch bezel (2).

### Installation Procedure

1. Install the door window switch (4) to the power lock and window switch bezel (2).
2. Install the power door lock switch (3) to the window switch bezel (2).
3. Connect the wire harness connector (1) to the power door window switch (4).
4. Connect the wire harness connector (1) to the power door lock switch (3).
5. Install the power lock and window switch bezel (2) to the door trim.
6. Install the screws (5).

## Front Door Switch Replacement Left, Pontiac Sedan

### Removal Procedure

1. Remove the screws (5).
2. Remove the power lock and window switch bezel (4) from the door trim.
3. Disconnect the wire harness connector (1) from the power door lock switch (2).
4. Disconnect the wire harness connector (1) from the power door window switch (3).
5. Remove the power door lock switch (2) from the window switch bezel (4).
6. Remove the door window switch (3) from the power lock and window switch bezel (4).

### Installation Procedure

1. Install the door window switch (3) to the power lock and window switch bezel (4).
2. Install the power door lock switch (2) to the window switch bezel (4).
3. Disconnect the wire harness connector (1) to the power door window switch (3).
4. Disconnect the wire harness connector (1) to the power door lock switch (2).
5. Install the power lock and window switch bezel (4) to the door trim.
6. Install the screws (5).

## Front Door Switch Replacement Right, Pontiac

### Removal Procedure

1. Remove the screws (2).
2. Remove the power lock and window switch bezel (1) from the door trim.
3. Disconnect the wire harness connector (3) from the power door lock switch (5).
4. Disconnect the wire harness connector (3) from the power door window switch (4).
5. Remove the power door lock switch (5) from the window switch bezel (1).
6. Remove the door window switch (4) from the power lock and window switch bezel (1).

### Installation Procedure

1. Install the door window switch (4) to the power lock and window switch bezel (1).
2. Install the power door lock switch (5) to the window switch bezel (1).
3. Connect the wire harness connector (3) to the power door window switch (4).
4. Connect the wire harness connector (3) to the power door lock switch (5).
5. Install the power lock and window switch bezel (1) to the door trim.
6. Install the screws (2).