For 1990-2009 cars

# SMU - SECTION 6A7 OIL PAN GASKET IS REUSABLE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6A7 - 2.3L ENGINE - OIL PAN GASKET IS REUSABLE

#### MODELS: 1988-93 PONTIAC GRAND AM 1988-91 OLDSMOBILE CUTLASS CALAIS 1992-93 OLDSMOBILE ACHIEVA 1988-93 BUICK SKYLARK 1988-93 CHEVROLET BERETTA WITH 2.3L ENGINE (VINS A, D, 3)

THE SERVICE MANUAL INCORRECTLY STATES THAT A NEW OIL GASKET SHOULD BE INSTALLED WHEN THE OIL PAN IS REMOVED.

THE OIL PAN GASKET USED ON 1988-94 2.3L ENGINES IS REUSABLE. THE GASKET ONLY NEEDS TO BE REPLACED WHEN THE GASKET IS DAMAGED.

IF AN OIL PAN IS REPLACED, ONLY REPLACE THE GASKET IF IT IS DAMAGED.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER." THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS OCCURRING ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993. GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.