For 1990-2009 cars

Caution: Provide additional support when a vehicle is on a hoist in the following ways:

• | Before removing parts, support the opposite end. This helps prevent the vehicle from slipping off.

• | Before removing major components, chain the vehicle frame to the hoist pads at the same end as the removal. This helps avoid a tip-off.

Failure to follow these precautions could cause vehicle damage, serious personal injury, or death.
1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the fuel pump electrical connector.
3. Lower the vehicle.
4. Start and run the engine until the fuel supply remaining in the fuel pipes is consumed. Engage the starter for 3.0 seconds in order to assure relief of any remaining pressure.
5. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Connect the fuel pump electrical connector.
7. Lower the vehicle.

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

8. Disconnect the negative battery cable in order to avoid possible fuel discharge if an accidental attempt is made to start the engine.