For 1990-2009 cars

# CLUNK NOISE : STEER INT. SHAFT INT. SHAFT SLIP JOINT MOTION

#### Models Affected: 1983-84 Century and Skylark

A "click" or "clunk" felt in the steering wheel during vehicle stops and starts may be caused by intermediate shaft slip joint motion. To correct this condition:

1. Remove intermediate shaft from car per Chassis Service Manual instructions.

2. Remove all foreign matter from shaft by wiping with a shop cloth.

3. Using chassis grease meeting requirements of GM-6031M (part mumber 1051344), grease the exposed shaft, FILL SHAFT POCKET AT POINT X and the inside of the tube at Point Y. See figure.

4. Fully compress intermediate shaft assembly two or three time to work grease into the assembly. REPEAT steps 3 and 4 three times.

5. Reinstall intermediate shaft assembly in car.

#### NOTE: When the intermediate shaft is reinstalled in the vehicle, care should be taken to assure the shaft boot seal is not dimpled or distorted. See figure. A distorted boot which rubs the intermediate shaft assembly may cause a slight steering bind when the vehicle is first operated in very cold weather.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.