For 1990-2009 cars

#### Tools Required

• | J 42137 Lock Plate Compressor

• | J 23653-SIR Steering Column Lock Plate Compressor

1. Install the inner race (5).
2. Install the upper bearing inner race seat (4).
3. Install the upper bearing spring (3).
4. Lubricate the turn signal cancel cam assembly (2) with lithium grease.
5. Install the turn signal cancel cam assembly (2).
6. Install the shaft lock (1).
7. Install the new bearing retainer using J 23653-SIR .
8. Install the SIR coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Assemble - Off Vehicle .