For 1990-2009 cars

# SMU - SECTION 10 - 7 - NEW REMOVE/INSTALL PROCEDURE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 10-7 - NEW REMOVE/INSTALL PROCEDURE FOR COUPE REAR QUARTER ARMREST

#### MODELS: 1996 BUICK SKYLARK 1996 OLDSMOBILE ACHIEVA (COUPE ONLY)

THIS BULLETIN ADDS THE REMOVAL AND INSTALLATION PROCEDURE FOR THE REAR QUARTER ARMREST (COUPE). PLEASE ADD THIS PROCEDURE TO SECTION 10-7 OF THE SERVICE MANUAL.

REAR QUARTER ARMREST - (BUICK AND OLDSMOBILE, COUPE) ====================================================

REMOVE OR DISCONNECT:

1. QUARTER TRIM PANEL, REFER TO "QUARTER TRIM PANEL - COUPE" IN SECTION 10-7 OF THE SERVICE MANUAL.

2. GLUE RETAINING REAR QUARTER ARMREST CLIPS TO QUARTER TRIM PANEL.

3. REAR QUARTER ARMREST.

INSTALL OR CONNECT:

1. REAR QUARTER ARMREST.

2. GLUE AT REAR QUARTER ARMREST CLIPS TO QUARTER TRIM PANEL.

3. QUARTER TRIM PANEL, REFER TO "QUARTER TRIM PANEL - COUPE" IN SECTION 10-7 OF THE SERVICE MANUAL.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.