For 1990-2009 cars

# INFO. ON RADIO ERROR CODE E14 WRAPPED TAPE ERROR

THIS IS A MONTHLY SERVICE NEWSLETTER ARTICLE. THIS BULLETIN IS NOT INTENDED FOR PUBLICATION.

#### SUBJECT: INFORMATION ON RADIO ERROR CODE E14 - WRAPPED TAPE ERROR

#### MODELS: 1995-98 BUICK SKYLARK 1995-98 BUICK PARK AVENUE/ULTRA 1995-98 BUICK LESABRE 1995-98 BUICK RIVIERA 1995-98 BUICK REGAL 1997-98 BUICK CENTURY WITH BUICK FAMILY OF RADIOS

CURRENT SERVICE INFORMATION DOES NOT ADDRESS RADIO CODE E-14. THIS CODE INDICATES A WRAPPED TAPE ERROR. THIS MEANS A TAPE IS WOUND UP IN THE TAPE PLAYER. THIS ERROR MESSAGE COULD BE CAUSED WITHOUT A TAPE BEING WRAPPED UP IF AN AFTERMARKET CD ADAPTER IS BEING USED, OR AN OLD/DAMAGED TAPE. THE CUSTOMERS SHOULD HAVE THE CODE AND CAUSES EXPLAINED TO THEM AS THE NEED ARISES.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.