For 1990-2009 cars

### Removal Procedure

1. Remove the guide bolt from the driver or the passenger seat shoulder belt.
2. Remove the side upper garnish molding from the windshield. Refer to Garnish Molding Replacement - Upper .
3. Remove the screws from the lower trim finish panel on the center pillar.
4. Remove the lower trim finish panel on the center pillar.

### Installation Procedure

1. Install the lower trim finish panel to the center pillar.
2. Install the screws to the lower trim finish panel on the center pillar.
3. Install the side upper garnish molding to the windshield. Refer to Garnish Molding Replacement - Upper .
4. Install the guide bolt to the driver or the passenger seat shoulder belt.