For 1990-2009 cars

# SERVICE MANUAL UPDATE REVISED FLYWHEEL TORQUE SPECS

THE REVISED FLYWHEEL BOLT TORQUE SPECIFICATION FOR THE 1990 - 91 A, C, E, H, N, AND W MODELS WITH 3800 (VIN L AND C) AND 3300 (VIN N) ENGINE IS LISTED BELOW:

FLYWHEEL BOLT TO CRANKSHAFT - 15 N.M + 50 DEGREES (11 LBS. FT. + 50 DEGREES)

TOOL REQUIRED: J36660 TORQUE ANGLE METER

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1991 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.