For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fender molding nuts | Fully Driven, Seated, Not Stripped
Fender molding screws | Fully Driven, Seated, Not Stripped
Fender to side rail bolts | 11 N·m | 97 lb in
Fender upper brace bolts | 4.5 N·m | 39.8 lb in
Grille and headlamp mounting support bolts | 10 N·m | 89 lb in
Hinge Pivot Bolt | 30 N·m | 22 lb ft
Hood hinge lower bolts | 27 N·m | 20 lb ft
Hood latch bolts | 30 N·m | 22 lb ft
Hood latch striker bolts | 30 N·m | 22 lb ft
Lower fender to rocker panel bolts | 11 N·m | 97 lb in
Upper hinge to hood bolts | 27 N·m | 20 lb ft