For 1990-2009 cars

# LABOR TIME GUIDE REVISION

THE LABOR TIME ALLOWANCES FOR LABOR OPERATIONS J1800, J1820, J1880, J0100 AND J0101 HAVE BEEN REVISED AS NOTED BELOW:

LABOR TIME ALLOWANCES:

1982-85 1982-84 1982-85 CENTURY SKYLARK RIVIERA VIN CODE R VIN CODE R VIN CODE Y

J1800 BLOCK, ENGINE FITTED REPL 10.9 10.5 J1820 ENGINE, PARTIAL/BASIC REPL. 8.9 8.5 J1880 ENGINE ASSEMBLY - REPLACE 6.6 6.2 J0100 MANIFOLD, EXHAUST-REPL. (RIGHT) 1.2 J0101 MANIFOLD, EXHAUST-REPL. (LEFT) .9

ADD: WITH AIR CONDITIONING .5 .5 WITH CRUISE CONTROL .2 .2

INCLUDES; TRANSFER ALL REQUIRED PARTS AND MAKE NECESSARY ARRANGEMENTS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.