For 1990-2009 cars

Notice: Handle the intake air temperature (IAT) sensor carefully. A damaged IAT sensor will affect proper operation of the fuel injection system.

### Removal Procedure

The IAT sensor is located on the air intake housing.

1. Remove the electrical connector.
2. Carefully grasp the sensor and with a twisting and pulling motion, remove the IAT sensor from air intake duct.

### Installation Procedure

1. Install the IAT Sensor into the hole.
2. Connect the electrical connector to the IAT Sensor.