For 1990-2009 cars

# BROKEN ENGINE STRUT BRACKET/ CYLINDER HEAD BRACKET BOLT

#### VEHICLES AFFECTED: 1982-85 'X' Car With 2.5L Engine and Manual Transmission 1983-85 'A' Car With 2.5L Engine and Manual Transmission

Customer comments of broken engine strut bracket and/or broken cylinder head bracket bolt mounting boss may be received on vehicles that have experienced a 'snap clutch' condition.

A service kit, P/N 14093564, has been released to improve the durability of the torque strut bracket and torque strut by limiting engine roll during hard transmission use conditions. The kit contains the following components:

P/N Description --- ----------- 14093563 Bracket 14065757 Bumper 6262213 Nut W/Washer 14093562 Assembly Instruction Sheet

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.