For 1990-2009 cars

### Removal Procedure

1. Remove the intermediate steering shaft. Refer to Steering Column Trim Cover Replacement - On Vehicle .
2. Remove the intermediate steering shaft seal from the front of the instrument panel.
3. Remove the intermediate steering shaft seal from the vehicle.

### Installation Procedure

1. Install the intermediate steering shaft seal to the vehicle.
2. Position the intermediate steering shaft seal on the front of the instrument panel.
3. Install the intermediate steering shaft. Refer to Steering Column Trim Cover Replacement - On Vehicle .